**Rangeline Engine Not Charging House Batteries**

**(No power to ignition wire)**

Remove black cover on B-pillar behind passenger side seat.

A picture containing indoor

Description automatically generated

This is where the Dodge side of the chassis battery hooks into Airstreams wiring. The wrong plug on our side was installed. Cut the blue wire off the plug. Pull Rams plug out and find the blue wire with a yellow tracer. Cut that wire and with a wago connector connect the two wires. Secure the Ram plug back into place.

Gain access to the Victron app. Pair to the DC/DC convertor by entering passcode 000000. Once paired to the DC/DC convertor go to settings. On the settings page there is a drop down menu called Function. Make sure that charger is selected in this drop box.

